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COS Down Under Assembly Instructions

	Kit Parts:

(1) Slide Rail

(10) #8 x Y2” Pan-Head Screws

(2) Recessed Bumpers

(2) #6 Wood Screws

(1) Wire Rack

(1) Shoulder Bolt

(2) Nylon Washers

(1) Rotating Arm Assembly

(2) Slide Guides

(1) SnapRackTM CD Rack

- (2 parts that snap together)
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Step 1 – Install the Slide Rail

Hold the Slide Rail on the bottom of the work surface to be mounted. Mark the hole locations for mounting. Please reserve the center screw hole on each end for the Recessed Bumpers. Remove the Slide Rail and pre-screw four (4) #8 x Y2” Pan-Head Screws into the work surface at both ends using the outside two holes, then remove. Next, hold the Slide Rail in place and mount four (4) #8 x Y2” Pan head Screws into the pre-screwed holes until flush, continue

placing the remaining six (6) mounting screws. (See Figure 1)

COS Down Under Assembly Instructions Step 3 – Assemble the Rotating Arm

Place one (1) Nylon Washer onto the Shoulder Bolt, then place the Shoulder Bolt through

the bottom of the Wire Rack. Please note: Wire Rack is in up position when the arc is a “U”. Place one (1) Nylon Washer onto the opposite end of the shoulder bolt. By hand, mount the Shoulder bolt into the end of the Rotating Arm Assembly, until it catches, then

using the Allen wrench, tighten until snug. Place one (1) Slide Guide on each end of the Rotating Arm Assembly. (See Figure 2)
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Step 4 – Install Rotating Arm Assembly to Slide Rail

Slide the Rotating Arm into the Slide Rail. Push all the way back until it stops. (See Figure 3)
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COS Down Under Assembly Instructions Step 5 – Install last Recessed Bumper

Using one (1) #6 Wood screw, mount the remaining Recessed Bumper in the center hole at the front end of the Slide Rail. (See Figure 1)
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Step 6 - Assemble the SnapRackTM CD Rack

Snap the two (2) sides of the CD rack together by lining up the snap detail at the bottom, making a “V” shape. Place in the wire rack assembly. (See Figure 4)
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Step 2 – Install Recessed Bumper


Using one (1) #6 Wood Screw, mount one (1) Recessed Bumper into the center screw hole at far end of Slide Rail, away from the front of the desk. This will keep the Rotating Arm Assembly from sliding out of the back of rail. (See Figure 1)�
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